**EQUIPMENT TYPE MOUNTING MOUNTING\_TYPE POWER LENGTH LIGHTING\_TYPE SHAPE FUEL\_TYPE**

Explosion Proof Lighting - Fluorescent, ceiling mounted, 2-40 W, 4' L

Explosion Proof Lighting - High pressure sodium, ceiling, pendent mounted, 100 W

Explosion Proof Lighting - Incandescent, ceiling mounted, 200 W

Explosion Proof Lighting - Metal halide, ceiling, pendent mounted, 200 W

Exterior Lighting - High pressure sodium, wall pack, 150 W

Exterior Lighting - Incandescent, wall mounted, 100 W

Exterior Lighting - Low pressure sodium, wall pack, 35 W

Exterior Lighting - Metal halide, wall pack, 175 W

Exterior Lighting - Quartz, wall mounted, 500 W

Interior Lighting, Fluorescent - Pendant Mounted (Type D)

Interior Lighting, Fluorescent - Recessed Fixture (Type C)

Interior Lighting, Fluorescent - Strip Fixture (Type A)

Interior Lighting, Fluorescent - Surface Mounted (Type B)

Interior Lighting, High Intensity - High Pressure Sodium 1000 W (Type F)

Interior Lighting, High Intensity - High Pressure Sodium 400 W (Type C)

Interior Lighting, High Intensity - Metal Halide 1000 W (Type G)

Interior Lighting, High Intensity - Metal Halide 400 W (Type B)

Interior Lighting, Incandescent - Recessed downlight w/baffles 150 W (Type B)

Interior Lighting, Incandescent - Recessed PAR-38 flood lamp w/louver 150 W (Type C)

Interior Lighting, Incandescent - Recessed R-40 flood lamp w/flat reflector 150 W (Type D)

Interior Lighting, Incandescent - Recessed reflector w/flat glass lens 150 W (Type A)

Emergency Lighting - Self-contained, fluorescent lamp pack

Generators - Diesel, 900 kW

Generators - Gas, 100 kW

Uninterruptible Power Supply - 7.5 kVA