**EQUIPMENT**  **SIZE**

Backflow Preventer - 1.5" pipe

**EQUIPMENT TYPE POWER SIZE FLOWRATE**

Booster Pump - 1 HP

Booster Pump - 1.5 HP

Booster Pump - Variable speed, 30 HP, 6" discharge, 1700 GPM

Booster Pump - Variable speed, 7.5 HP, 4" discharge, 400 GPM

**EQUIPMENT TYPE FLOWRATE**

Heat Transfer Package - One pump system, 55 GPM

Heat Transfer Package - One pump system, 130 GPM

Heat Transfer Package - Two pump system, 255 GPM

Heat Transfer Package - Two pump system, 35 GPM

**EQUIPMENT TYPE CAPACITY SIZE LOA**

Storage Tank - Galvanized steel, 135 gallon, 24" diameter, 75" L.O.A.

Storage Tank - Galvanized steel, 15 gallon, 14" diameter, 26" L.O.A.

Storage Tank - Glass lined, PE, 1330 gallon, 66" diameter, 107" L.O.A.

Storage Tank - Glass lined, PE, 140 gallon, 24" diameter, 80" L.O.A.

**EQUIPMENT FUEL\_TYPE CAPACITY POWER FLOWRATE**

Water Heaters, Commercial, Electric - 350 gal, 180 KW, 738 GPH

Water Heaters, Commercial, Electric - 500 gal, 30 KW, 123 GPH

Water Heaters, Commercial, Gas - 155 MBH input, 150 GPH

Water Heaters, Commercial, Gas - 175 MBH input, 168 GPH

Water Heaters, Commercial, Oil - 201 gal, 1500 MBH input, 1441 GPH

Water Heaters, Commercial, Oil - 221 gal, 300 MBH input, 288 GPH

**EQUIPMENT SIZE**

Sanitary Waste Separator - 3" size